[Cover]
Test title:       
Device name:      
Device version:   
Test operator:    
Institution:      
Date/time:        6 avr. 2009 11:08:02
API version:      2,40
Driver version:   2,40
Firmware version: 1
Software version: 1.10
Hardware version: 1.10
Notes/comments: 

[Settings]
Conformance tester:      auto-start; 20,00 Mbits/second
Loop-back device:        disabled; 200,00 Mbits/second; spilling
Loop-back timecodes:     non-compliant; no loopback
UUT disconnect delay:    17 microseconds
UUT link recovery time:  17 microseconds
Default NCHAR:    255
Default timecode: 42

[Bit-level]
Test:   Determine Link State
Status: Success
Result: UUT is link enabled
Note:   See Waveform panel for updated waveform trace

Test:   Link Initialisation Test
Status: Success
Result: Link initialisation was correct
Note:   Used UUT error response delay (UUT_delta) of 17 microseconds

Test:   Start Up Link Speed
Status: Success
Result: Startup rate within (10 Mbits/second +/- 1 Mbit/second)
                  Measurement     Accuracy  Minimum         Maximum
   Bit-to-bit:    10,00 +/- 0,14      0,14   9,86 +/- 0,14  10,14 +/- 0,14
   Rise-to-rise:  10,00 +/- 0,07      0,07   9,93 +/- 0,07  10,07 +/- 0,07
   Fall-to-fall:  10,00 +/- 0,07      0,07   9,93 +/- 0,07  10,07 +/- 0,07
Note:   Measurement duration 13,10 microseconds (131 bits)
Note:   Average link rate 10,00 Mbits/second
Note:   All rate measurements are in Mbits/second
Note:   See Waveform panel for updated waveform trace

Test:   Start Up Waveform
Status: Success
Result: Valid start-up waveform 011101000
   D: 01110100010001000100010001
   S: 11011110111011101110111011
Note:   See Waveform panel for updated waveform trace

Test:   Link Shutdown Analysis
Status: Success
Result: Valid shutdown time (100,00 +/- 1,39 ns < 555 ns)
Note:   See Waveform panel for updated waveform trace

Test:   Disconnect Timeout
Status: Success
Result: Timeout within valid range of 727 to 1000 ns inclusive
Note:   Checked transmit bit periods from 450 to 1280 ns
Note:   Used UUT link recovery time 600 microseconds (UUT_recovery)
Note:   Disconnect timeout is between 870 and 1000 ns (+/- 10 ns)
Note:   Used 2000 iterations per time step
Note:   Upper limit of timeout might be non-compliant

Test:   Simultaneous D/S Transition Check
Status: Success
Result: No simultaneous D/S transitions detected.
Note:   Test duration 10,05 seconds
Note:   See Waveform panel for updated waveform trace

[Exchange]
Test:   Validate ErrorWait
Status: Success
Result: All tests passed
   Response to parity error: correct: moved to ErrorReset
   Response to ESC-EOP:      correct: moved to ErrorReset
   Response to ESC-EEP:      correct: moved to ErrorReset
   Response to ESC-ESC:      correct: moved to ErrorReset
   Response to FCT:          correct: moved to ErrorReset
   Response to NCHAR:        correct: moved to ErrorReset
   Response to TCODE:        correct: moved to ErrorReset
   Test parameters:          UUT_delta = 17 us, NCHAR = EOP+EOP, timecode = 42

Test:   Validate Ready
Result: One or more tests failed
   Response to parity error: correct: moved to ErrorReset
   Response to ESC-EOP:      correct: moved to ErrorReset
   Response to ESC-EEP:      correct: moved to ErrorReset
   Response to ESC-ESC:      correct: moved to ErrorReset
   Response to FCT:          failed:  did not move to ErrorReset
   Response to NCHAR:        correct: moved to ErrorReset
   Response to TCODE:        correct: moved to ErrorReset
   Test parameters:          UUT_delta = 17 us, NCHAR = EOP+EOP, timecode = 42
Note:   UUT might be in Started or Connecting not Ready when test was run so
Note:   the results might be unreliable


Test:   Validate Started
Status: Failed
Result: One or more tests failed
   Response to parity error: correct: moved to ErrorReset
   Response to ESC-EOP:      correct: moved to ErrorReset
   Response to ESC-EEP:      correct: moved to ErrorReset
   Response to ESC-ESC:      correct: moved to ErrorReset
   Response to FCT:          failed:  did not move to ErrorReset
   Response to NCHAR:        correct: moved to ErrorReset
   Response to TCODE:        correct: moved to ErrorReset
   Test parameters:          UUT_delta = 17 us, NCHAR = EOP+EOP, timecode = 42
Note:   UUT might be in Connecting not Started when test was run so the
Note:   results might be unreliable

Test:   Validate Connecting
Status: Success
Result: All tests passed
   Response to parity error: correct: moved to ErrorReset
   Response to ESC-EOP:      correct: moved to ErrorReset
   Response to ESC-EEP:      correct: moved to ErrorReset
   Response to ESC-ESC:      correct: moved to ErrorReset
   Response to FCT:          correct: did not move to ErrorReset
   Response to NCHAR:        correct: moved to ErrorReset
   Response to TCODE:        correct: moved to ErrorReset
   Test parameters:          UUT_delta = 17 us, NCHAR = EOP+EOP, timecode = 42

Test:   Validate Run
Status: Success
Result: All tests passed
   Response to parity error: correct: moved to ErrorReset
   Response to ESC-EOP:      correct: moved to ErrorReset
   Response to ESC-EEP:      correct: moved to ErrorReset
   Response to ESC-ESC:      correct: moved to ErrorReset
   Response to one FCT:      correct: did not move to ErrorReset
   Response to NCHAR:        correct: did not move to ErrorReset
   Response to TCODE:        correct: did not move to ErrorReset
   Test parameters:          UUT_delta = 17 us, NCHAR = EOP+EOP, timecode = 42

[EOP/EEP]
Test:   Empty Packet (EOP)
Status: Success
Result: Did not disconnect (correct)
   Empty EOP packets sent:       8

Test:   Empty Packet (EEP)
Status: Success
Result: Did not disconnect (correct)
   Empty EEP packets sent:       8

Test:   Empty Packet Loop-back (EOP)
Status: Success
Result: Did not disconnect (correct)
   Empty EOP packets sent:       8
   Empty EOP packets received:   0
   Empty EEP packets received:   0

Test:   Empty Packet Loop-back (EEP)
Status: Success
Result: Did not disconnect (correct)
   Empty EEP packets sent:       8
   Empty EEP packets received:   0
   Empty EOP packets received:   0

Test:   Send Packet With EEP
Status: Success
Result: Successfully transmitted the packet
   Packet transmitted (hexadecimal): 
      (empty) <EEP>
   Packet received (hexadecimal): 
      00 01 02 03 04 05 06 07 08 09 0a 0b 0c 0d 0e 0f 10 11 12 13 14
      15 16 17 18 19 1a 1b 1c 1d 1e 1f 20 21 22 23 24 25 26 27 28 29
      2a 2b 2c 2d 2e 2f 30 31 32 33 34 35 36 37 38 39 3a 3b 3c 3d 3e
      3f 40 41 42 43 44 45 46 47 48 49 4a 4b 4c 4d 4e 4f 50 51 52 53
      54 55 56 57 58 59 5a 5b 5c 5d 5e 5f <EEP>

[Timecode]
Test:   Investigate UUT timecode support
Status: Success
Result: UUT supports timecodes
Note:   UUT did not return any timecodes

Test:   Timecode/NCHAR confusion
Status: Success
Result: Packet and timecode sent: please check arrival at UUT
Note:   UUT ought to have received a single-byte packet 255 and timecode 42.
Note:   If UUT received a two-byte packet <255 42> it is treating timecodes
        as NCHARs which is wrong.

Test:   UUT receives valid timecodes
Status: Success
Result: Timecode 1 sent: please check arrival at UUT

Test:   UUT ignores invalid timecodes
Status: Success
Result: Timecode 21 sent: please check ignored by UUT

Test:   Measure timecode frequency
Status: Success
Result: Time codes received and UUT did not disconnect
   60 ticks received (60 valid, 0 invalid)
   Measured tick frequency = 541666,67 Hz
   Minimum tick frequency  = 83333,33 Hz
   Maximum tick frequency  = 1000000,00 Hz

[Credit]
Test:   FCT Overflow Check
Status: Success
Result: All tests passed
   Response to  1 FCT:          correct: did not move to ErrorReset
   Response to  2 FCTs:         correct: did not move to ErrorReset
   Response to  3 FCTs:         correct: did not move to ErrorReset
   Response to  4 FCTs:         correct: did not move to ErrorReset
   Response to  5 FCTs:         correct: did not move to ErrorReset
   Response to  6 FCTs:         correct: did not move to ErrorReset
   Response to  7 FCTs:         correct: did not move to ErrorReset
   Response to  8 FCTs:         correct: moved to ErrorReset
   Response to  9 FCTs:         correct: moved to ErrorReset
   Response to 10 FCTs:         correct: moved to ErrorReset
   Response to 11 FCTs:         correct: moved to ErrorReset
   Response to 12 FCTs:         correct: moved to ErrorReset
   Response to 13 FCTs:         correct: moved to ErrorReset
   Response to 14 FCTs:         correct: moved to ErrorReset
   Response to 15 FCTs:         correct: moved to ErrorReset
Note:   Require silent UUT or TLI at least half the UUT rate

Test:   NCHAR (EOP) Overflow Check
Status: Failed
Result: UUT didn't disconnect
Note:   See Waveform panel for updated waveform trace
Note:   Require TLI link rate to be at least 8 times the UUT link rate
        Average TLI link rate 20,00 Mbits/second
        Average UUT link rate 20,00 Mbits/second
        UUT link rate too high relative to TLI link rate
Note:   Success might be due to empty packet handling not NCHAR credit error

Test:   NCHAR (EEP) Overflow Check
Status: Failed
Result: UUT didn't disconnect
Note:   See Waveform panel for updated waveform trace
Note:   Require TLI link rate to be at least 8 times the UUT link rate
        Average TLI link rate 20,00 Mbits/second
        Average UUT link rate 20,00 Mbits/second
        UUT link rate too high relative to TLI link rate
Note:   Success might be due to empty packet handling not NCHAR credit error

Test:   Empty Packet Credit Check
Status: Failed
Result: UUT incorrectly ignores empty packets (or its receiver is full)
Note:   UUT appears to have a 49 byte receive buffer
Note:   UUT must consume all packets sent to it

Test:   UUT Credit Error Check
Status: Success
Result: No credit errors detected

[Packet (1)]


[Packet (2)]


[Other]
Test:   Started 12.8 microsecond timeout
Status: Success
Result: Valid timeout duration (11,640 < 12,700 < 14,330 microseconds)
Note:   Result ignores transmitter start-up but includes transmitter shutdown
        time so it might not be an accurate measure of the UUT timeout.

Test:   Connecting 12.8 microsecond timeout
Status: Success
Result: Valid timeout duration (11,640 < 13,100 < 14,330 microseconds)
Note:   Result ignores transmitter start-up but includes transmitter shutdown
        time so it might not be an accurate measure of the UUT timeout.

Test:   Maximum Bit Period
Status: Success
Result: Maximum bit period within valid range of 727 to 1000 ns
Note:   Maximum bit period is 950 ns (+/- 10 ns)

Test:   NULL Arrival Times
Status: Success
Result: Success
Note:   Edge at time 20,92 microseconds from 41,52 to 39,55 microseconds
Note:   Edge at time 20,96 microseconds from 39,55 to 37,58 microseconds
Note:   Edge at time 21,00 microseconds from 37,58 to 35,62 microseconds
Note:   Edge at time 21,04 microseconds from 35,62 to 33,65 microseconds
Note:   Edge at time 21,08 microseconds from 33,65 to 31,68 microseconds
Note:   Edge at time 21,12 microseconds from 31,68 to 29,71 microseconds
Note:   Edge at time 21,16 microseconds from 29,71 to 27,74 microseconds
Note:   Edge at time 21,20 microseconds from 27,74 to 25,78 microseconds
Note:   Edge at time 21,24 microseconds from 25,78 to 23,81 microseconds
Note:   Edge at time 21,28 microseconds from 23,81 to 21,84 microseconds
Note:   Edge at time 21,72 microseconds from 22,20 to 24,38 microseconds
Note:   Edge at time 21,76 microseconds from 24,38 to 26,55 microseconds
Note:   Edge at time 21,80 microseconds from 26,55 to 28,73 microseconds
Note:   Edge at time 21,84 microseconds from 28,73 to 30,90 microseconds
Note:   Edge at time 21,88 microseconds from 30,90 to 33,08 microseconds
Note:   Edge at time 21,92 microseconds from 33,08 to 35,26 microseconds
Note:   Edge at time 21,96 microseconds from 35,26 to 37,43 microseconds
Note:   Edge at time 22,00 microseconds from 37,43 to 39,61 microseconds
Note:   Edge at time 22,04 microseconds from 39,61 to 41,78 microseconds
Note:   Edge at time 22,08 microseconds from 41,78 to 43,96 microseconds
Note:   Unable to identify second ErrorReset segment
Note:   First ErrorWait segment isn't horizontal
Note:   First ErrorReset (dy)   =   6,12 microseconds
Note:   Average ErrorReset      =   6,12 microseconds
Note:   First  ErrorReset slope =   1,23, intercept 18,10 microseconds
Note:   ErrorWait slope         =      ?, intercept ? microseconds
Note:   ErrorWait+Tx(null)      =   0,00 microseconds
Note:   Early null dip is not deep enough
Note:   Early null dip width    =   0,00 microseconds
Note:   Used UUT link recovery time 600 microseconds (UUT_recovery)

Test:   Error Recovery Time
Status: Success
Result: Link recovery time within expected range of 18.46 to 22.55 microseconds
Note:   Used UUT link recovery time 600 microseconds (UUT_recovery)
Note:   Link recovery time is between 21.8 and 21.84 microseconds (+/- 0.1)
Note:   Number of test iterations: 10000

